|  |  |  |
| --- | --- | --- |
| No’s | Description | Requirement |
| 1 | Type | Reciprocating |
| 2 | Free air Delivery | 250 to 300 Cub meter per hour |
| 3 | Max. Pressure | 40 bar |
| 4 | Operating Pressure | 30 bar |
| 5 | Cooling system | Forced air Cooled |
| 6 |  |  |
| 7 | Engine | Diesel Driven |
| 8 | Stroke | 4 Stroke |
| 9 | Speed | 1500 -1800 RPM |
| 10 | Number of Cylinders | 4 or 6 |
| 11 | Starting method | Battery Starter motor Type |
| 12 |  |  |